<http://projects.ict.usc.edu/mxr/faast/>

**Installation**

To use FAAST, you will need to download and install the following software:

1. [OpenNI Unstable Build for Windows v1.0.0.25](http://www.openni.org/downloadfiles/openni-binaries/20-latest-unstable)
2. [PrimeSense NITE Unstable Build for Windows v1.3.0.18](http://www.openni.org/downloadfiles/openni-compliant-middleware-binaries/33-latest-unstable)  
   During NITE installation, enter the free license key from OpenNI: **0KOIk2JeIBYClPWVnMoRKn5cdY4=**
3. Hardware drivers for your sensor (only one of the following)
   * Microsoft Kinect: [SensorKinect Module](https://github.com/avin2/SensorKinect" \t "_blank) – download Win32 installer from Bin folder
   * PrimeSensor: [PrimeSensor Module](http://www.openni.org/downloadfiles/openni-compliant-hardware-binaries/31-latest-unstable" \t "_blank) – this does **NOT** work with the Kinect